-Replace with original
-Register any name and make sure to use the same serial method but input anything eg: 0000-0000-0000-0000-80 (serial ends in 80 as stated on the screen)


---------------------------------------------------------------------------